0.0-1.01.0z(m)

1.02.0r(m)

Close fitting , conducting shell + large array of active feedback coils to stabilize external, internal modes.

IBW pondermotive feedbackfor the external kink.

Scrapeoff-layer current modulationand edge biasing for external modes.

Lower hybrid + mode conversion launchers for localized, modulated current drive, shear flow stabilization.NBI modulation (perpendicular and tangential) for internal modes.

Fig. 1