Is-IsIs-Is

-IsIs(+)(-)(-)(-)

BIASING

SEGMENTED

DIVERTOR

STRIKE LINE

OF SOL

UNSEGMENTED

PLASMA

COLUMN

(+) BORON NITRIDE

SHIELDS

(b)Fig.1b Upper outer divertor toroidally segmented into separate electrodes with bias of opposite polarity applied to each segment.Fig.1a View of strike side of a toroidally segmented divertor for twisting the magnetic field lines in the outer scrape-off layer so as to broaden the effective deposition area of the incident outer strike points.

EFFECTIVE

STRIKE AREA

SPIKES ON SOL

PROJECTION

VIEW OF STRIKE SIDE OF SEGMENTED DIVERTOR(a)

INITIAL