¥˚Fake Rotating Shell Network (by R. Fitzpatrick and T. Jensen) can be implemented by measuring the spacial difference of the toroidal phasingHelical flux leakage sensor loop and fake rotating shell approach

¥˚Sensors located front & back of "thick alminum shell" assesses the advantage of the "thick highly conducting first wall" like ITER

fake rotation direction helicalflux leakagesensor toroidal directionDfFig. 4