57 MHZ FOLDED WAVEGUIDE FOR FSXORNL/PPPL

Fig.1. View of ORNL Folded Waveguide. The gate valve and duct allow the waveguide to be removed while torus is under vacuum and adjusted for polarization changes or oriented for IBW or Fast Wave operation.