Fig.2b. Poloidal current streamlines a t a fixed time halo feedback calculations with halo width WH = 0.01. The other parameters for these runs were TH = 20 eV, a = 266, EMAX = 40 V/m and TV = 0.1 eV. Streamlines deep inside the plasma region are not shown.