BIASING

SEGMENTED

DIVERTOR

STRIKE LINE

OF SOL

UNSEGMENTED

PLASMA

COLUMN

(+)IsIsIs

(+)(+)(-)

BORON NITRIDE

SHIELDS

Fig.1. Toroidally segmented upper outer divertor for feedback control of SOL currents. Bias is applied to different segments by the feedback stabilization control system.