25.4 cm(10") SCALE

DF-2DF-3

FSX Divertor Design Concept ¥ Deep ITER-Like Vertical Targets, Baffled, Low Fueling, Biasable, Flexible

(+)(-)

INNER & OUTER CHANNEL

BIASING BUSES

VERTICAL GRAPHITE TARGET

304-SS WITH

MICA BACKING

TO FLOAT

CHANNELS

OUTER BAFFLE

DOME BAFFLE

-10 SUPPORTS -

SPACIOUS DOME REGION

BETWEEN SUPPORTS

AVAILABLE FOR

PUMPING OPTION

¥ Reference Equilibrium: Double-Null, TF =1.5T, Ip = 660KA, IDF-3 = 1KA.¥ Increasing IDF-3 Adjusts Strike Points Away from X-Point.

10 TOROIDAL UNITS, CONVENIENTLY REPLACABLE Fig. 3. FSX Divertor Design Concept